enable

conf t

hostname SW-01

enable secret TempleWater-123#

banner motd "ACESSO APENAS PARA O DEPTO. DE TI DA WATER TEMPLE LTDA."

username linkdoti privilege 15 secret hey-listen-3\*

ip domain-name watertemple.local

crypto key generate rsa general-key modulus 1024

line vty 0 15

transport input ssh

login local

exit

line console 0

login local

exit

service password-encryption

vlan 10

name ADMINISTRACAO

vlan 20

name RH

vlan 30

name TI

vlan 40

name SERVIDORES

vlan 50

name WI-FI

interface vlan 30

ip add 172.16.0.109 255.255.255.240

interface range f0/1

no shutdown

switchport mode access

switchport access vlan 10

interface range f0/2

no shutdown

switchport mode access

switchport access vlan 20

interface range f0/3

no shutdown

switchport mode access

switchport access vlan 30

interface range f0/23

no shutdown

switchport mode access

switchport access vlan 50

interface f0/24

switchport mode trunk

switchport trunk native vlan 99

switchport trunk allowed vlan 10,20,30,40,50,99

interface range f0/4-22

shutdown

interface range g0/1-2

shutdown

do wr